Exemplar Problem

Text

Description automatically generated

Solution

(b) calculate angular frequency, and use the sinusoidal function of AC current.