**Ques**: A 10 mF capacitor is connected with an ac source E = 200 2 sin (100 t) V through an ac ammeter (it reads rms value) . What will be the reading of the ammeter?

Solution:

